N1MM+ Call History Installation Instructions

First, download the latest .txt file from here:  

http://www.cqp.org/software/CQP-CH-N1MM-05Oct2018.txt

Then:
1. Upgrade N1MM+ to the latest version.

2. Open N1MM+ and go to File --> Import --> Import Call History

3. Select the previously downloaded pre-fill file and click "Open".  The callsigns will be imported.  

Note: If you look at the bottom of the main Entry Window after the importing process is complete, you'll see how many callsigns have been imported. ("X,XXX callsigns imported”).

4. To activate the Call History function go to the Config Menu and highlight “Enable Call History Lookup".  A checkmark will appear next to “Enable Call History Lookup”.

5. Restart N1MM+ Logger

Now when you type in a callsign in the Entry Window and hit the Space Bar, you should see the EXCH field filled in automatically for any callsign listed in the Call History file. For example:  
N6ZFO will show LAKE for the EXCH 
K6T will show TEHA
K6EI will show SIER

Note: It's important to use the Space Bar and NOT the Tab key to get this working properly.

Hope this helps.  GL in CQP this weekend.

73
John, K6MM